# Dell Quad Port 1 Gigabit Broadcom 5720 Network Daughter Card, CusKit

Dell Part 540-BBHG

The BCM5720 is a fully integrated 10/100/1000BASE-T Gigabit Ethernet media access control and physical layer transceiver solution for high-performance network applications. The Quad-Port Gigabit Network Daughter Card features quad triple-speed IEEE 802.3-compliant Media Access Controllers (MACs) with quad 10/100/1000 Ethernet transceivers (PHYs), PCI Express bus interface, and on-chip memory buffer in a single device. It's based on dual BCM5720 Controllers each providing two ports.

## Media

### Why should I buy a Dell Upgrades over a third-party part?

### Tested and Verified Tier-1 OEM-Grade Parts

Ensure compatibility with Dell servers, storage and networking

### Ease of Installation

Save time with Dell Upgrades that are shipped as kits with the necessary hardware and firmware.

### Secure Supply Chain Focus

Protect system data and integrity with parts sourced from a secure supply chain

### Dell Tech Support and Warranties

Preserve Dell technical support and warranties—which do not support systems with third-party upgrades

### Compatibility

This product is compatible with the following systems:

- PowerEdge R620
- PowerEdge R630
- PowerEdge R640
- PowerEdge R720
- Poweredge R720xd
- PowerEdge R730
- PowerEdge R730XD
- PowerEdge R740
- PowerEdge R740XD
- PowerEdge R7425
- PowerEdge R820
- PowerEdge R840
- PowerEdge R920
- PowerEdge R930
- PowerEdge R940
- PowerEdge R940xa
- PowerVault DL4000
- PowerVault DR4100
- PowerVault DX6112 SN
- PowerVault NX3240
- PowerVault NX3340

The BCM5720 is a fully integrated 10/100/1000BASE-T Gigabit Ethernet media access control and physical layer transceiver solution for high-performance network applications. The Quad-Port Gigabit Network Daughter Card features quad triple-speed IEEE 802.3-compliant Media Access Controllers (MACs) with quad 10/100/1000 Ethernet transceivers (PHYs), PCI Express bus interface, and on-chip memory buffer in a single device. It's based on dual BCM5720 Controllers each providing two ports.

- Provides x1 PCIe interface
- Features a compact space-saving design
- Ideal for high-performance network applications