USB-C to USB3.0A, RJ45, HDMI and USB-C

**Overview**

This is a USB-C 4-in-1 hub with HDMI, USB-A，RJ45 and Type-C female port, providing an ideal solution for extending the port of Type-C/Thunderbolt 3 host (PC/Laptop/Mobile phone, etc.), especially for those host with a single USB-C port. This hub adopts the latest DP1.4 Alt mode supported IC, enabling to output HDMI video with max 4k/60Hz and at the meanwhile transfer USB 3.1 data with max 5Gbps. RJ45 helps host to get access to super-fast Ethernet network. Besides, the USB-C female supports PD 3.0 with max 100W PD Charging when connecting a PD Adapter and supports max 5Gbps data transmission when connecting a USB-C device. It can work on all DP Alt mode supported Type-C host.

**Features**

* Operation systems supported: Windows XP/Vista/Win 7/8/8.1/10/Mac OS 10.5 or later
* Thunderbolt 3 Compatible
* Power delivery at up to 100W
* HDMI Resolution up to 4k60Hz
* Network speeds at up to 1 Gbit/s

****

**Technical Specification**

|  |  |  |  |
| --- | --- | --- | --- |
| **Model** | *USB3.1CCOM16* | **Specs** | *Internet speed up to 1 Gbit/s**HDMI supports up to 4096x2160 60Hz 4:4:4 Support 60Hz HDR and HDCP 2.2 support* |
| **Length** | *0,15m* |  |  |
| **Material** | *PVC Cable* |  |  |
| **Shielding** | *Single shielded* | **Warranty** | *30 Years* |
| **Common applications** | *For signal between computer / notebook and monitor.* | **Version** | *HDMI Version 2.0, PD version 3.0* |
|  | *Used to expand the available ports on your notebook/laptop* |  |  |
|  |  | **Testing** | *Tested before shipment* |
|  |  |  |  |
| **Colors** | *Black* | **Packing** | *Microconnect Polybag* |
|  |  | **Certifications** | *CE, FCC* |
|  |  | **Installation and use** | *Plug and Play* |
|  |  |  | *Indoor* |

****